CT / Nidec Links

**“Connect Software” – (connection from PC to the drive to setup parameters and run):**

<https://acim.nidec.com/en-us/drives/control-techniques/products/software/commissioning/unidrive-m-connect>

**“CTScope” – (useful tool for trending, tuning and debugging)**

<https://acim.nidec.com/en-us/drives/control-techniques/products/software/commissioning/ctscope>

Notes / Comments:

* May need to setup an email account to download (see below)



* Choose the Connect Software Bundle
* Connect a direct Ethernet cable to the drive (and your PC)
	+ The drive is typically shipped with the following IP address: 192.168.1.101
* Use CTScope for tuning and debugging